Security Gate Selection DF

Sample Tender Document Entry

Security gate with rotating flaps
Motor-driven security gate, consisting of a sensor-monitored lane with electronically controlled motor-driven waist-high turning gates for use in open or closed operating modes.
Two-way operation with entrance and exit in one lane in the closed operating mode

Body and cover in V2A stainless steel, matt finished or sanded and coated with acid protection. 10 mm transparent Perspex barrier elements. 10 integrated opto-sensors per lane for monitoring and protection against unauthorized access without valid ID or by following authorized persons.
An integrated control unit controls opening and closing of the rotating flaps. In case of contact of the barrier elements with obstacles, the barrier elements stop immediately.
At the front and back of the security gate body, trapeze-shaped elements can accommodate card readers as well as lane indicators and/or release signals.

Reference Product: Gotschlich Model Selection DF

with the following built-in options:
•	Opto-sensors for detection of misuse by climbing over
•	Opto-sensors for detection of misuse by crawling under
•	Lane indicators in the trapeze elements
•	Light signal for indication of granted access or blocking in the relevant direction, built into lid
•	Factory installation of customer-provided card readers